**Procedure for Dehorning Using the Callicrate Bander**

1. Place the loop over the horn furthest from you. Ensure you do not drag the loop along the bottom side of the horn as you pull it towards the base. (This will cause the loop to roll. If the loop rolls on the horn, it will likely return to its original shape thus rolling back toward the tip of the horn.
2. Once the loop is in the proper position, surrounding 1-2cm of skin from the horn base, pull the bander and loop toward you. This will keep the loop close to the head and in the hairline at the horn base.
3. Tighten the loop until the tension peg on the bander touches the back of the slot.
4. Press the crimping lever until it will go no further, to prevent the loop from slipping and releasing tension.
5. Cut the loop as close to the spool as possible.
6. Figure eight duct tape around the horns (over the loops)\*\*
7. Repeat procedure on other horn.

\*\*Duct tape helps to protect the rubber loops